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Product Guide Specification
Specifier Notes:  This product guide specification is written according to the Construction Specifications Institute (CSI) 3-Part Format, including MasterFormat, SectionFormat, and PageFormat, as described in The Project Resource Manual—CSI Manual of Practice, Fifth Edition.

This section must be carefully reviewed and edited by the Architect or Engineer to meet the requirements of the project and local building code.  Coordinate this section with other specification sections and the Drawings.  Delete all “Specifier Notes” after editing this section.

Section numbers are from MasterFormat 2010 Update.

SECTION 26 05 34
WIRING DUCT

Specifier Notes:  Delete any information below in Parts 1, 2 or 3 which is not required or relevant for the project.

PART 1 – GENERAL

1.01	SUMMARY

A.	Section Includes: Wiring duct for routing and concealing wiring in control panels.
	
1.02	REFERENCES

	A. 	Underwriters Laboratories, Inc (UL):
		1. 	UL 1565		Positioning Devices

	B. 	Canadian Standard Association (CSA):
		1.	CSA C22.2 No. 18.5	Positioning Devices
	2.	CSA C22.1		Canadian Electrical Code Part I (CEC)

	C.	National Fire Protection Association (NFPA)
			1.  	NFPA 70	 	National Electrical Code (NEC)

1.03	SUBMITTALS

	A.	Comply with Section 01 33 00 – Submittal Procedures.

	B.	Product Data:
1. 	Submit manufacturer’s descriptive literature and product specifications for each product.
2. 	Manufacturer’s product drawings. 

1.04	QUALITY ASSURANCE

A.	Manufacturer Qualifications: Products shall be free of defects in material and workmanship. 

B.	Furnished products are listed, recognized or classified by third party agencies as suitable for the intended purpose.

1.05 WARRANTY

A. Product is warranted free of defects in material and workmanship.

B. Product is warranted to perform the intended function within design limits.

PART 2 – PRODUCTS

2.01	GENERAL 

A.	Standard wiring duct shall be available in the following constructions:
1. 	Solid wall wiring duct: TY___SP_6 series
	2. 	Wide slot wiring duct: TY___WP_6 series
	3.	Narrow slot wiring duct: TY___NP_6 series
	4.	Round hole wiring duct: TY___RP_6 series

B.	Halogen-free wide slot wiring duct shall be series TY___WHW6.

C.	Wiring duct shall be UL Recognized to UL 1565 and CSA Certified to C22.2 No. 18.5.

2.02	MANUFACTURERS

A.	Acceptable Manufacturers:
		ABB Installation Products Inc. 
860 Ridge Lake Boulevard
Memphis, Tennessee 38120
800-816-7809, 901-252-5000
electrification.us.abb.com

		Product: 	Ty-Duct® Wiring Duct

2.03	DESIGN AND PERFORMANCE REQUIREMENTS

A.	Standard wiring duct shall have a UL94V-0 flame rating and a 50ºC maximum continuous use temperature.

B.	Standard wiring duct shall be available in the following colors:
	1.	gray
	2.	white
	3.	black
	4.	intrinsic blue

C.	Halogen-free wiring duct shall have a UL94V-1 flame rating and a 95ºC maximum continuous use temperature.

D        	Halogen-free wiring duct shall be available in white.

E.       All wiring duct shall be available in slot widths of 0.75” to 6”.

F.       All wiring duct shall be available in slot depths of 1” to 5”.

G.       All wiring duct shall be available in 6 foot lengths.

PART 3 – EXECUTION

3.01	INSTALLATION

A. 	Installation shall be in accordance to the NEC, CEC and manufacturer’s instructions where
 	applicable.
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